В архиве 4 файла: 

1) in_!mpg123.dll
2) in_CDReader.dll 
3) HQSoftProc_SoftwareResamping_v46.exe
4) kxdrv3538l-full.exe

Первые два файла нужно переместить в папку плагинов винампа, обычно эта папка находится C:/Program Files/Winamp/Plugins/
Затем установите HQSoftProc_SoftwareResamping_v46.exe
и выставите рекомендуемые тут http://forum.academ.org/index.php?showtopic=167272&view=findpost&p=3410193
настройки.
Для того, чтобы всё работало, нужно удалить встроенные плагины винампа:
in_cdda.dll и in_mp3.

С вопросами обращайтесь по ICQ - 225438945 или пишите ЛС на форуме(http://forum.academ.org/index.php?showuser=891)

  Ваш Пётр_Сергеевич. :)

*Так же рекомендуется вместе родных драйверов для SB LIve!, Audigy1/2/4+, использовать альтернативные kxdrv3538l-full.exe - они дадут больше возможностей и улучшат звучание. Для этого нужно сперва удалить родные дрова, а потом поставить альтернативные.*

Описание плаг-инов:
1) покамест нет

2) 
	What is CD Reader plugin?
	~~~~~~~~~~~~~~~~~~~~~~~~~
CD  Reader  is  a  freeware  WinAmp  plugin  to play music CDs with exceptional
quality.

	Why CD Reader better than standard WinAmp CD plugin ?
     	~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
Here is why:
1. Improved read quality, much closer to 100%.
2. Ability to use quality DAC of your audiocard. (Many CD-ROMs have only
   12-bit DAC)

	About 1st clause.  All players play  CDs by reading  data sectors once,
one by one, continuously. No any  reread on defect sectors occurs. This  caused
by many reasons. Method of playing CDs was born when maximum available  reading
speed was 1x.  It's a very  hard to find  CDDA sector to  reread it, because of
poor CDDA navigation system (original  guaranteed precision is about 0.5  sec).
Computer program  using good  6x CD  drive can  eliminate these  obstacles. So,
read quality can approach  to 100%. You can  ask: "How about my  Data-CDs? It's
all read  fine on  my CD-ROM.  And how  CD-ROM reread  sectors on my Data-CDs?"
That's true. But  thanks to improved  Data-CD navigation system  and additional
error correction layer.  Difference is huge,  here is about  100Mb of efficient
data payoff.

	How is it work ?
	~~~~~~~~~~~~~~~~
	CD Reader plugin uses RAW_READ function (also known as 'read long')  to
extract digital  audio data  from CD.   So, your  CD-ROM drive  must have  such
capability. CD Reader plugin can use  two low level interfaces to perform  this
function - ASPI  and Win32. ASPI  is Windows 95/98  embedded interface. Windows
NT have not this interface installed  by default.  However, you can  install it
separately.  From  other  hand  Windows  NT  have naitive low level interface -
Win32, you  can use  it without  installing any  additional software. But, some
CD-ROMs does  not support  RAW_READ function  thru Win32  and do  well it  thru
ASPI.
	No any  position de-jittering  performed.   All code  relies on  modern
CD-ROM drives and  drivers. Because, most  of old CD-ROM  drives which able  to
read raw  data from  media, unable  to do  it on  sufficient (real  time, 1x at
least) speed.

	How to use it?
	~~~~~~~~~~~~~~
	Be   sure   you   use   WinAmp   2.0   or   higher.  Then  simply  copy
'in_CDReader.dll'  to  WinAmp\Plugins  directory.   Don't  forget  to   shutoff
original  WinAmp   CD  plugin   by   changing   its  extension,   for   example
'in_cdda.dll.off'.  Now  you  can  try  to  play  CD.  If "Your CD-ROM does not
support RAW_READ function" dialog  box appears - bad  luck, you can't use  this
plugin. If player report "Buffer size too big to handle", try to reduce  buffer
size down to one  sector. Some CD-ROMs capable  of read CDDA only  by 1 sector.
More sectors in buffer - better  skip protection, less CPU use.   Fewer sectors
- faster  seek response  and more  CPU use.  If you  have more than one CD-ROM,
ensure  to  set  right  "ASPI  device"  option  in setup. You can get faltering
sound. This caused  by poor read  speed that in  its turn can  be caused by bad
media or CD-ROM drive.

	CDDB
	~~~~
	In this version of CD Reader  plugin is able to read information  about
CD in drive from CDDB Internet server which contain song names and other  stuff
for wide variety of  CD's. Click on CDDB  tab to make CDDB  settings. CD Reader
plugin is  able to  cache CD  information. To  enable this  feature click  'Use
local CDDB'  checkbox. Cached  information will  be kept  in cdplayer.ini  file
which located in main Windows folder.

	License agreement
	~~~~~~~~~~~~~~~~~
None of the executable modules or the documentation of CD Reader plugin may  be
modified in any way.

All rights to  CD Reader plugin  belong  to  Vladimir Kopjov. You  may use this
product  only  in  accordance  with  the  restrictions  listed  in this license
agreement.

CD  Reader  plugin  is  distributed  on  the  "AS-IS"  principle  without   any
warranties or pledges.

This software may be used freely only with WinAmp(tm),  and may not be  copied,
sold,  distributed  or  used  for  any  other purpose without the prior written
Vladimir Kopjov's consent.

The author bears  no responsibility for  any damage or  loss of data  resulting
from the use or misuse of CD Reader plugin.

The author does not assume any  obligation to inform anyone about new  versions
of the software, nor about any additions or modifications.

The use of  CD Reader plugin  means nothing more  than your acceptance  of this
license agreement.

	Support freeware
	~~~~~~~~~~~~~~~~
	Really like this plugin ? You can support the author by sending _any_
music CD (may be one you want to throw out) to:
	620144
	55 Kuibyshev st.
	Ekaterinburg, Russia
	PARAD Vladimir Kopjov

	Contacts
	~~~~~~~~
	E-mail:	copah@parad.ru
	WWW:	http://www.url.ru/~copah/
-----------------------------------------------------------------------------------------------------------------------
3) Version 4.6 Pro
HQSoftProc Software Resampling Plugin
created by Adrian Paul

Freeware Plugin!

USE THIS SOFTWARE AT YOUR OWN RISK !!!
I will not be responsible for anything regarding the 
use of this software!

If you are not looking for highest audio quality or have 
no idea about what distortion is, than this component is 
of no use for you ... it will only make your CPU work 
more on music...

This plugin is specially inteded to be used for SBLive!, 
Audigy, Audigy2 series of soundcards as they have the
biggest issues when resampling audio to their internal
DSP working samplerate. This plugin is the only way
to hear the soundcard playback without distortion, and
resampling distortion on SBLive! is quite huge, while
for Audigy series of soundcards it was very little
improved. Also this plugin can feed the required stream
to kernel streaming plugins.

Don't get me wrong that if you do not have SBLive! or
Audigy you are kept away from this issue: nope, all
soundcards that have DSP on them have to resample all
incoming data to their working samplerate, and generally
the Resamplings of these cards are not of high quality due
to the hardware need of limitations.

The previous version of this plugin was known under the
name of "SBLive! Resampling Problemfix" or 
"SBLive! Resampling Bugfix" or "Software Resampling".

Now this project (and the new ones) has a website
www.HQSoftProc.go.ro, where I will keep you posted
with the workprogress of the plugin and the new projects.


[The SBLive!/Audigy issue]

   SBLive! and Audigy1/2 soundcard's DSP work at 48KHz,
so a big problem here for 44.1KHz streams.
   SBLive! has a low quality resample to 48KHz algoritm.

This is the SBLive! (and not only) problem:

   absolutely any audio stream is converted to 48KHz 
(for Audigy1/2 it is converted to 48KHz or 96KHz or 192KHz
if not using DSP - see below note)
   the worst performance is 44.1KHz audio streams (cd audio).

   Audigy has the same issue even if it is promoted
as a 192KHz/24bit soundcard (please note the important *,
* means that 192KHz is in 2 channels only, and 96KHz
is in 6 or 8 channels, BUT with DSP disabled, that is
with absolutely no effects loaded (not even bass and treble),
so if you use at least one effect or bass/trebe than Audigy2
will switch to DSP and process everything to 48KHz.

 1.393% IMD Distortion at 15KHz for Audigy2 
(check www.tomshardware.com for details)

[The solution:]

   my high quality resample to 48KHz 
(or any frequency>= 48000, that means 96KHz and 192KHz too).

Testing results:

 using SBLive! to resample to 48000:
	19KHz IMD=20%
	18KHz IMD=10%
	16KHz IMD=5%
	14KHz IMD=1%
 You don't believe me ...???? I've included in component pack generated tones
used in my test versions of 44100Hz and 48000Hz ... Should sound the same !!!

 using my component for KernelPrecision=100 (that means kernelsize 16000 samples
at resampling to 48000Hz):
	19KHz IMD=0.01%
	18KHz IMD=0.001% ; can't measure less than this
	16KHz IMD=0%

CPU Load: 
<35% on Duron 825MHz for KernelPrecision 100
<22% on Duron 825MHz for KernelPrecision 50
<15% on AthlonXP2000+ for KernelPrecision 120

[known issues]
Can't resample to a lower samplefrequency than the input.

[configuration items] 

<TargetSampleRate> specifies resample target frequency of filter (should be
48000 for SBLive!/Audigy1/2 cards if used in DSP mode, or 96000 for Audigy1/2
if not used in DSP mode, and this must be the working Samplerate of the DSP 
on your soundcard!!!

Note: for Audigy2 in 2 channel mode and no DSP you can set this to 192KHz

<KernelPrecision> is a coeficient to calculate the filter kernel size of the
lowpass filter in the multirate filter, for keeping the same quality of the
filtering regardless of the input samplerate. From my tests I would recommend
50 to be the absolute minimum, but I left the option to enter a lower value
for people with slower machines. More than 300 is useless as it can't improve higher.

altering this results:
	higher KernelPrecision => higher quality more CPU load.
	lower KernelPrecision  => lower quality less CPU load.
don't alter this if you do not know what means this or if you do not check
the results on a spectrum analyzer!

[some hints]
If you really want your SBLive/Audigy/Audigy2 to sound perfect I recommand you
to download and install KX Drivers wich you can find at: www.kxproject.com.
These drivers are freeware.
  Best sound : KX Drivers + HQSoftProc SoftwareResampling plugin. Try it!
  Best results for any soundcard:
   MAD plugin + HQSoftProc SoftwareResampling + KernelStreaming plugin
    or mpg123                                 + ASIO plugin

[recommended setup]
1. for Audigy1/2 with DSP disabled:
   at least 150 KernelPrecision
   96000 Output samplerate (for Audigy2 in 2channels mode use 192KHz if you 
don't use KX drivers and, of course no DSP)
   24bit output bitdepth
   32bit output bitdepth for MAD plugin (does not allow FP->16bit conversion,
but to FP->32bit integer)
   64bit floating point for Shibatch mpg123 plugin (audio stream passed directly
to the output plugin, without roundings)
   use KX drivers (at least 3538i), but be aware to use 
WaveHQ and disable DSP in "24/96 Router", or if you want ASIO, you can use
ASIO4ALL in combination with setting in KX ASIO control panel the ASIO Format
to 24bit/96khz 8+8. If using different format in KX ASIO then make sure you setup
the output plugin with the same settings as in KX ASIO control panel (e.g. if
want to use 16/48KHz setup my plugin to output to 48KHz and 32bit)

2. for SBLive! and Audigy1/2 in DSP mode:
   150 KernelPrecision
   48000 Output Samplerate
   32bit output bitdepth (matches internal processing of SBLive bitdepth)
   32bit output bitdepth for MAD plugin (to improve rounding)
   use KX drivers

Please note that some versions of the Creative drivers don't handle 32bit properly 
so you have to switch to 16 bit or 24 bit.

[Contact:]
	email: adi111p@yahoo.com
	web:   www.HQSoftProc.go.ro


P.S. Haven't you noticed that DVD movies (sampled to 48000Hz) sounded perfect
on your sound system and Audio CD's didn't????? This is why!

another advice: Use KX drivers for SBLive and Audigy and Audigy2 soundcards. You will get
professional EQ-s, filters, 5.1,6.1,7.1 Decoders, but you will need some time to understand 
how to configure it

download it from www.kxproject.com


[History]
v4.6 (2006.04.29)
- added 64bit floating point input (useful for Shibatch mpg123 input plugin)
- different approach on stream passing to the output plugin

v4.4 (2005.08.29)
- fixed CanWrite call from Winamp, this should fix the bug reported
  by Smash Maniac, the issues with Winamp DSP plugins, and improve
  handling of winamp
- changed readme file with latest infos, and fixed a line that was
  left from the old plugin readme file

v4.3 (2005.05.24)
- fixed compiler issue and gained performance (CPU usage was reduced by
  approx. 50%)
- fixed some bugs
- reduced memory allocation to exactly the size needed

v4.2
- reworked internal processing and handling of the channels streams
  now works for up to 10 channels, 8,16,24,32bits input, 16,24,32 output
- internal processing set to 64bits floatingpoint
- fixed bugs in playback redirection to a winamp plugin
- found a good formula to compute the required amplification of the
  signal after resampling, to get the same volume level as the input
- added a peak engine that reduces the volume as the processed 
  output would exceed levels (clipping) and lowers the level accordingly
  so no clipping will occur again on that stream. (by default is reduced
  to 80% the level because of the processing,but that is not allways ok)

v3.2 
- found a bug when computing filterkernel

v3.15 Pro
- changed name to "HQSoftProc Resampling plugin"
- created webpage for this project and the incoming ones
  at www.HQSoftProc.go.ro
- small improvements in the ergonomy of the configuration interface
- new ThumbNail of the plugin for Winamp site

v3.103 Pro
- rebuilt BufferEngine, now you can use crossfading output plugins
- fixed ocasional crashes

v3.1 Pro
- Added button "Open Readme.txt for details ..." in configuration
- Changed About box

v3 Pro
- changed name from "SBLive! Resampling bugfix" to "Software Resampling Plugin"
  beacause this plugin is designed for Audigy1/2/SBLive! boards, 
  but also for other DSP-based soundcards
- Added multiple input stream bitdepth: 16/24/32bits
  now you can use MAD plugin with 24/32bit output
- Added configurable output bitdepth: 16/24/32bits
- Removed Directsound output, instead you can configure wich output plugin to use
  so now the sound processed by softwareresampling is redirected to an existing
  winamp output plugin
- fixed some synchronization bugs in engine
- finally fixed vis sync problems because of the new BufferEngine, that is used
  to redirect resampled stream to an existing winamp output plugin

v1.2
- bugfix: Shoutcast streams not working
- bugfix: crashes when playing using CDDA
- bugfix: vis sync problems
- improvements: internal computation is done in 64bit now (32bit were before
  the improvement) at the cost of small CPU computation power cost (5-20% increase)
- for Audigy 2 use 96000KHz and at least 18000 kernel size

v1.1
- bugfix: volume control is ok now
- bugfix: if paused and changing track no sound played

v1.01
- software conversion memory handling rebuilded

v1.0 
- added configuration

v0.0 first build
- no configuration
- seek plops
---------------------------------------------------------------------------------------------------------------------